;
LanguageName=
;
;
0000="File",
0001="Exit",
0002="Exit the application",
0003="Error",
0004="Language Update Failed",
0005="Open",
0006="Load binary file",
0007="Save",
0008="Save data for backup",
0009="Tools",
0010="Select Device",
0011="Config",
0012="Configure the target",
0013="Detect Chip (F1)",
0014="Detect chip ID",
0015="Read from chip (F2)",
0016="Read data from target",
0017="Verify data (F3)",
0018="Verify the data between memory and target",
0019="Blank Check (F5)",
0020="Check if the target is blanked",
0021="Erase chip (F4)",
0022="Erase the memory block on the chip",
0023="Write chip (CTRL+W)",
0024="Write data to target chip",
0025="Activation",
0026="Activate the software based on hardware ID",
0027="Help",
0028="About",
0029="About GQBLaster ....",
0030="Goto Configure folder",
0031="Open configuration folder",
0032="   Speed: ",
0033="Test Module Not Loaded",
0034="No Hardware",
0035="Auto Script",
0036="Script Directory",
0037="Select Script Directory",
0038="Type",
0039="No",
0040="Yes",
0041="Address",
0042="New",
0043="Clear",
0044="View XML",
0045="Duplicate Test Name",
0046="Email Activate",
0047="Online Activation",
0048="Hardware ID",
0049="Email Address",
0050="Activation Code",
0051="Please enter your email address",
0052="USB Not connected",
0053="USB connected (1.1)",
0054="USB connected (2.0)",
0055="Target: ",
0056="Warning!!",
0057="Are you sure you want to program?  ",
0058="Are you sure you want to erase?  ",
0059="Erase time",
0060="Program time",
0061="Unknown device",
0062="Read speed",
0063="Compare data Failed address",
0064="Check memory range.",
0065="Time",
0066="Save binary file",
0067="Compare data OK",
0068="Command unknown ",
0069="Write speed",
0070="Program Starts...",
0071="Flash blanked",
0072="Flash is not blank at address",
0073="Incompatible  adapter(top module) detected.",
0074="Busy",
0075="Erase starts...",
0076="Message Log",
0077="Copy",
0078="Copy the current selection's contents to the clipboard",
0079="Paste",
0080="Paste the clipboard's contents into the current position",
0081="Usage: initusb\r\n Reinit the USB port.",
0082="Usage: exit\r\n Exit the application.",
0083="Usage: help (cmd)\r\n Output the usage of the command.",
0084="Usage: detect\r\n Detect the devices.",
0085="Usage: read address length\r\n Usage:read\r\n Read memory from target to PC memory",
0086="Usage: verify address length\r\n Usage:verify\r\n compare memory between target and PC memory",
0087="Usage: write \r\n Write memory to target from PC memory",
0088="Usage: save tabname (filename)\r\n save start end (filename)\r\n Save the data in the tab",
0089="Usage: load (filename)\r\n Load file into memory.",
0090="Usage: about\r\n Display version info",
0091="Usage: cls\r\n Clear the output display",
0092="Usage: configshow\r\nShow Existing config.",
0093="Usage: erase address length\r\n Usage:erase\r\n Erase the flash",
0094="Usage: blkchk address length\r\n Usage:blkchk \r\n Blank check flash",
0095="Usage: speed 0 (1) (2)\r\nAdjust target speed",
0096="Usage: log (1) 0\r\n Enable/disable the log.",
0097="Usage: color ffffff\r\n Change back ground color",
0098="Usage: script \r\nDisplay all the script files\r\n script file\r\n Display script",
0099="Script file error!",
0100="No script files",
0101="Please select",
0102="Please select right value",
0103="Exit Script",
0104="Press enter to continue.Spacebar and enter to break....",
0105="Bad command",
0106="Script finished",
0107="Clear command window",
0108="Language",
0109="Select new language",
0110="Language Selection",
0111="Available Language",
0112="Usage: config (target)",
0113="loaded",
0114="File Error",
0115="Wrong target selected",
0116="Recent Files",
0117="Recent Targets",
0118="(Not Activated)",
0119="(Activated)",
0120="Clear output window",
0121="Device Selection/Search",
0122="Search Device For",
0123="Manufacture",
0124="Device",
0125="My Favorite Devices",
0126="Package",
0127="Adapter",
0128="Programmer",
0129="Tips: Always search for exact part number first. Then choose the closest part number.",
0130="Select",
0131="Cancel",
0132="Target not exist",
0133="Stop",
0134="Stop access target",
0135="Usage: devices\n Display all the devices",
0136="Usage: program address length\r\n Usage:program\r\n program target.",
0137="Not enough data",
0138="Usage: device \r\n select device",
0139="Init",
0140="Fill the memory tab with initial value",
0141="Saved",
0142="Registration",
0143="Register the software based on hardware ID",
0144="Register",
0145="Name",
0146="Edit Device File",
0147="Usage: d address.\r\n Make the address visible",
0148="Please wait...",
0149="Duplcaite found",
0150="Nand verify considers ECC algorithm !!",
0151="New Flash",
0152="New Chip",
0153="Start a new chip operation",
0154="Usage: blankbbt \r\n Build bad block table for blank chip (Erase first)",
0155="Blank BBT",
0156="Build bad block table for blank chip (Erase first)",
0157="Usage: srcbbt \r\n Build bad block table for source chip (file)",
0158="Source BBT",
0159="Build bad block table for source chip (file)",
0160="Save BBT",
0161="Save bad block table",
0162="Load BBT",
0163="Load bad block table",
0164="Usage: savekbbt \r\n Save bad block table",
0165="Usage: loadbbt \r\n Load bad block table",
0166="Usage: mfc \r\n Multiple Read File Correction",
0167="Multiple File Correction",
0168="Multiple Read File Correction",
0169="Usage: ctf \r\n Create target file based on target bad block table",
0170="Create target file",
0171="Create target file based on target bad block table",
0172="Need at least two files",
0173="Target File",
0174="Target BBT File",
0175="Size does not match",
0176="Smart copy",
0177="Copy to target with analyze",
0178="Failed, Stop script",
0179="Error, Stop script",
0180="Unsupported page size",
0181="Erase the chip first",
0182="Make sure the proper source file is loaded",
0183="ID detection error, check pin connetion!!",
0184="Are you sure?",
0185="Create temporary file",
0186="Target bad block No. ",
0187="Source bad block No. ",
0188="Start Block:",
0189="Number of Blocks:",
0190="Copy source badblock",
END
